# mpls topology-driven-lsp ip-interfaces

#### Syntax

[ no ] mpls topology-driven-lsp ip-interfaces [ egress | ingress ]
[ { access-list | prefix-list } listName ] [ host-only ]

no mpls topology-driven-lsp ip-interfaces [ egress | ingress ] [ host-only ]
[ policy-list ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies LSPs to be put into the IP routing table for forwarding plain IP traffic. The no version removes the LSPs from the table.

| Note: This command is deprecated and may be removed completely in a future release. The function provided by this command has been replaced by the ldp ip-forwarding command.

#### Options

- egress—Has no effect
- ingress—Has no effect
- access-list—Specifies that listName is an access list
- prefix-list—Specifies that listName is a prefix list
- listName—Name of access list or prefix list that specifies LSPs over which IP interfaces are created
- host-only— Specifies that only LSPs to host addresses are added to the IP routing table
- policy-list—Removes previously applied access lists or prefix lists

#### Mode

Global Configuration