# redundancy revert

#### Syntax

[ no ] redundancy revert slotNumber
[ startTime [ [ startMonth startDay | startDay startMonth ] startYear ] ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Forces the router to revert to the primary line module in the specified slot. If you specify a time or time and date, reversion occurs when the primary line module becomes available after that time. Otherwise, reversion occurs immediately. Issuing this command causes reversion once; after reboot, the router returns to the settings configured in the software. The no version has no effect.

#### Options

- slotNumber—Number of the slot in which the primary line module resides
- startTime—Time, in 24-hour format (00:00:00), at which the router reverts to this line module
- startMonth—Name of the month in which the router reverts to this line module
- startDay—Day of the month on which the router reverts to this line module
- startYear—Four-digit year in which the router reverts to this line module

#### Mode

Privileged Exec