# Monitoring the Configuration of Scheduler Profiles

#### Purpose

Display information about scheduler profiles. If you do not specify the scheduler profile name, data for all scheduler profiles is displayed.

You can display the values that you configured using a QoS parameter for assured rate, shaping rate, and shared-shaping rate.

#### Action

To display information about all scheduler profiles:

    host1#show scheduler-profile
                shaping                     strict
    scheduler    rate     burst   weight   priority   assured rate
    ---------   -------   -----   ------   --------   ------------
    default     <none>    32767     8         no      <none>
    wf100       128000    32767     20        no      75000
    spSV25      5000000   32767     40        no      64000
    videoHar    <none>    32767     8         no      hierarchical

To display the number of times that a QoS profile references the scheduler profile:

    host1#show scheduler-profile brief
    scheduler-profile default referenced 39 times in qos-profiles
    scheduler-profile wf100 referenced 1 time in qos-profiles
    scheduler-profile spSV25 referenced 2 times in qos-profiles

To display a list of QoS profiles that reference the scheduler profile:

    host1#show scheduler-profile references
    scheduler-profile default
      Referenced by QoS profiles:
        atm-default
        serial-default
        ethernet-default
        server-default

    scheduler-profile wf100
      Referenced by QoS profiles:
        ipV610

    scheduler-profile spSV25
      Referenced by QoS profiles:
        qospro25

#### Meaning

Table 40 lists the show scheduler-profile command output fields.

Table 40: show scheduler-profile Output Fields

Field Name | Field Description
--- | ---
scheduler | Name of the scheduler profile
shaping rate | Maximum bandwidth, in bits per second, provided to a node or queue
burst | Catch-up number associated with the shaper
weight | HRR weight of a node or queue
strict priority | Status of strict priority, yes or no
assured rate | Desired bandwidth, in bits per second, provided to a node or queue, or the keyword, hierarchical, to indicate that HAR is used
Referenced by QoS profiles | QoS profiles that reference this profile

#### Related Documentation

- Configuring a Scheduler Hierarchy
- Configuring Simple Shared Shaping
- Configuring Compound Shared Shaping
- show scheduler-profile