# committed-action

#### Syntax

For IP and IPv6 rate-limit profiles:

[ no ] committed-action { drop | transmit | mark markVal }

For L2TP rate-limit profiles:

[ no ] committed-action { drop | transmit }

For MPLS rate-limit profiles:

[ no ] committed-action { drop | transmit | mark-exp expValue }

For hierarchical rate-limit profiles:

[ no ] committed-action { drop | transmit [ conditional | unconditional | final ] }

#### Release Information

Command introduced before JunosE Release 7.1.0.
conditional, unconditional, and final keywords added in JunosE Release 7.2.0.

#### Description

Sets the action for packets conforming to the committed rate and committed burst size and conforming to the exceed rate and exceed burst size for a rate-limit profile. The no version restores the value to the default value, drop.

#### Options

- drop—Drops the packet
- transmit—Transmits the packet; for hierarchical rate limits:
  - conditional—Packets must pass the next rate limit
  - unconditional—Packets take resources, but are not affected by the rest of the hierarchy
  - final—Packets exit the hierarchy at rate limit
- markVal—Value in the range 0–255
- expValue—EXP bit value in the range 0–7

#### Mode

Rate Limit Profile Configuration

#### Related Documentation

- Creating a Two-Rate Rate-Limit Profile