Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# route-map

#### Syntax

Specifying a route map for DVMRP or RIP:

[ no ] route-map mapTag [ interfaceType interfaceSpecifier ]

Defining a route map:

[ no ] route-map mapTag [ permit | deny ] [ sequence ]

Defining a route map for data MDTs:

route-map routeMapName

no route-map

#### Release Information

Command introduced before JunosE Release 7.1.0.
IP PIM Data MDT Configuration mode added in JunosE Release 8.2.0.

#### Description

Specifies a route map for DVMRP, RIP, or data MDTs, or defines the conditions for applying routing policies to filter or modify routes redistributed into or propagated by a routing protocol. The no version deletes the route map.

#### Options

- mapTag—String of up to 32 alphanumeric characters.
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- mapTag—String of up to 32 alphanumeric characters. The redistribute Router Configuration command uses this string to reference this route map. Multiple route maps may share the same map tag.
- permit—If the match criteria are met for this route map and permit is specified, the route is redistributed as controlled by the set actions.
- deny—If the match criteria are met for the route map and deny is specified, the route is not redistributed, and no further route maps sharing the same map tag are examined.
- sequence—Number, in the range 0–65535, that indicates the position a new route map is to have in the list of route maps already configured with the same map tag. If given with the no version of this command, it specifies the position of the route map that should be deleted.

#### Mode

Address Family Configuration (RIP), Global Configuration, IP PIM Data MDT Configuration

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out