# bgpGracefulRestart

#### Description

BGP Graceful Restart Feature log

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

None

#### Warning Log

None

#### Notice Log

Log BGP performed or did not perform a graceful restart; router supports or does not support non-stop forwarding; router is capable of switching gracefully, deferring, or resuming best path selection decision process; BGP routes allowed or prevented from being downloaded to line cards; graceful-restart timer expiration; marking or removing stale routes; waiting to receive end-of-rib marker from peer; received end-of-rib marker from all peers

#### Info

None

#### Debug

Standby SRP will wait for BGP convergence on next restart

#### Filter 1

access-class—This filter is not currently supported

#### Filter 2

peer—This filter is not currently supported

#### Filter 3

route-map—This filter is not currently supported

#### Filter 4

router—See description of the bgpRoutes router filter for information about this filter

#### Filter 5

in—This filter is not currently supported

#### Filter 6

out—This filter is not currently supported