# bgpMessages

#### Description

BGP protocol messages

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

None

#### Warning Log

Unknown message type received; invalid field in received message; notification message received or sent; invalid capability length in received ORF capability; invalid capability value in received ORF capability; invalid ORF in received ORF capability; ORF entries exceeded maximum limit in received prefix list

#### Notice Log

Open message received or sent; update message received or sent; route-refresh message received or sent; route-refresh-cisco message received or sent; received ORF capability; received route refresh message with ORF entries

#### Info

None

#### Debug

Keepalive message received or sent (Full decode of message logged if verbosity is high)

| Note: Send messages are logged to the bgpMessages log when a message is added to the send queue. A debug message is logged to the bgpConnections log when the message is actually passed to TCP.

#### Filter 1

access-class—This filter is not currently supported

#### Filter 2

peer—See description of the bgpRoutes peer filter for information about this filter

#### Filter 3

route-map—This filter is not currently supported

#### Filter 4

router—See description of the bgpRoutes router filter for information about this filter

#### Filter 5

in—Matches on traffic coming into the router

#### Filter 6

out—Matches on traffic going out of the router