# ppp multilink multiclass

#### Syntax

ppp multilink multiclass [ multilink-classes classNumber ]

no ppp multilink multiclass [ multilink-classes ]

#### Release Information

Command introduced in JunosE Release 11.1.0.

#### Description

Enables multiclass MLPPP on the router, and optionally creates a specified number of multilink classes. The no version without the multilink-classes keyword disables multiclass MLPPP on the router. The no version with the multilink-classes keyword restores the number of multilink classes to the default value, 1.

#### Options

- classNumber—Number of multilink classes that can be created in the range 1–8, with a default value of 1.

#### Mode

Interface Configuration, Profile Configuration, Subinterface Configuration

#### Related Documentation

- Enabling Multiclass MLPPP
- Configuring Multiclass MLPPP