# ip dhcp-local auto-configure agent-circuit-identifier

#### Syntax

[ no ] ip dhcp-local auto-configure agent-circuit-identifier

#### Release Information

Command introduced in JunosE Release 7.3.0.

#### Description

Configures the DHCP local server to support the creation of dynamic subscriber interfaces built over dynamic VLANs that are based on the agent-circuit-id option (suboption 1) of the option 82 field in DHCP messages. This command is specific to a virtual router. The no version disables the autoconfigure feature.

#### Mode

Global Configuration