# exception monitor

#### Syntax

exception monitor ipAddress [ directoryName ]

no exception monitor

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables the core dump monitor and specifies the location to which the router transfers core dump files. The no version disables the core dump monitor.

#### Options

- ipAddress—IP address of the server to which you want the router to transfer core dump files
- directoryName—Name of the directory on the server to which you want the router to transfer core dump files

#### Mode

Global Configuration