# frame-relay keepalive

#### Syntax

frame-relay keepalive [ seconds ]

no frame-relay keepalive

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables the LMI mechanism for serial lines using Frame Relay encapsulation. The no version disables this capability. The keepalive command is similar to the frame-relay lmi-t391dte command.

#### Options

- seconds—Number in the range 5–30; default value is 10 seconds; defines the keepalive interval; the interval must be set, and the value on the DTE should be less than the value set on the DCE

#### Mode

Interface Configuration