# baseline bridge interface vpls

#### Syntax

baseline bridge interface vpls vplsName

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Sets a statistics baseline for a VPLS instance on the VPLS virtual core interface, which represents all of the MPLS tunnels from the router to the remote VPLS edge (VE) devices. The router implements the baseline by reading and storing the statistics at the time the baseline is set and then subtracting this baseline whenever baseline-relative statistics are retrieved. There is no no version.

| Note: Using the baseline bridge interface vpls command affects the VPLS virtual core interface, but has no effect on the network interfaces associated with the VPLS instance. To set a statistics baseline for a VPLS network interface, use the baseline bridge interface command.

#### Options

- vplsName—Name of a VPLS instance created with the bridge vpls transport-virtual-router command

#### Mode

Privileged Exec

#### Related Documentation

- Setting a Baseline for VPLS Statistics in the JunosE BGP and MPLS Configuration Guide