# instance-interface-type

#### Syntax

instance-interface-type {instanceInterfaceType | set | superset }

no instance-interface-type { instanceInterfaceType | all }

#### Release Information

Command introduced in JunosE Release 7.1.0.
lag keyword added in JunosE Release 8.1.0.

set and superset keywords added in JunosE Release 9.2.0.

#### Description

Assigns an instance-interface type to a QoS parameter definition. Instance-interface types indicate the interfaces for which QoS clients can assign QoS parameter instances. You can specify up to eight instance-interface types for each parameter definition. The no version removes the specified instance-interface type from the parameter definition.

#### Options

- instanceInterfaceType—One of the following instance-interface types: atm, atm-vc, atm-vp, bridge, ethernet, fr-vc, ip, ip-tunnel, ipv6, lag, l2tp-session, l2tp-tunnel, lsp, pppoe, serial, server-port, svlan, vlan
- set—Specifies an interface set as an instance-interface type
- superset—Specifies an interface superset as an instance-interface type
- all—Removes all instance-interface types

#### Mode

QoS Parameter Definition

#### Related Documentation

- Configuring a Basic Parameter Definition for QoS Administrators
- Creating a QoS Parameter on an Interface Superset or Interface Set