# ip dhcp-local limit

#### Syntax

ip dhcp-local limit
{ atm | ethernet | pos | vlan | interface InterfaceType InterfaceSpecifier } value

no ip dhcp-local limit [ atm | ethernet | pos | vlan
| interface InterfaceType InterfaceSpecifier ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
interface keyword and interfaceType and interfaceSpecifier variables added in JunosE Release 7.1.0.

pos keyword added in JunosE Release 10.0.0.

#### Description

Specifies the maximum number of IP addresses that the DHCP local server can supply to each VPI/VCI, VLAN, Ethernet subnetwork, or POS access interface, or to a particular interface or subinterface. The no version restores the default address limit value, 48000.

#### Options

- atm—Specifies the limit for VPIs and VCIs
- ethernet—Specifies the limit for Ethernet subnets
- pos—Specifies the limit for POS access interfaces
- vlan—Specifies the limit for VLANs
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- value—Maximum number of leases, in the range 0–96000; default is 48000

#### Mode

Global Configuration