# ip proxy-arp

#### Syntax

ip proxy-arp [ restricted | unrestricted ]

no ip proxy-arp

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables proxy ARP on an Ethernet or bridge1483 interface. Proxy ARP is enabled by default. The no version disables proxy ARP on an Ethernet or bridge1483 interface.

#### Options

- restricted—Restricts proxy-arp to hosts on the local interface
- unrestricted—Enables proxy-arp for all reachable hosts

#### Mode

Interface Configuration, Subinterface Configuration