# nsf interface wait

#### Syntax

[ no ] nsf interface wait [ seconds ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the maximum amount of time, in seconds, that an IS-IS process on a restarting router waits for all interfaces with IS-IS adjacencies to come up before completing the restart process. The no version restores the default maximum wait time, 10 seconds.

#### Options

- seconds—Maximum wait time, in the range 5–120 seconds, before the IS-IS restart process is completed; default value is 10 seconds

#### Mode

Router Configuration