# baseline ip udp

#### Syntax

baseline ip udp [ vrf vrfName ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets a statistics baseline for UDP statistics. The router implements the baseline by reading and storing the statistics at the time the baseline is set and then subtracting this baseline whenever baseline-relative statistics are retrieved. There is no no version.

#### Options

- vrfName—Name of the VRF; string of 1–32 alphanumeric characters

#### Mode

Privileged Exec