# frame-relay lmi-n391dte

#### Syntax

frame-relay lmi-n391dte keepExchanges

no frame-relay lmi-n391dte

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets the full-status polling counter (N391) on a DTE interface. The no version restores the default value, assuming an LMI has been configured.

#### Options

- keepExchanges—Number in the range 1– 255; default value is 6; number of keep exchanges to be done before requesting a full-status message. If you specify a value of 1, you receive full-status messages only.

#### Mode

Interface Configuration