# debounce-time

#### Syntax

debounce-time interval

no debounce-time

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets the interval to wait before bringing up a RIP interface that was brought down. The no version restores the default value, 10.

#### Options

- interval—Seconds in the range 0–60

#### Mode

Address Family Configuration, Router Configuration