# l2c line-configuration

#### Syntax

l2c line-configuration interface interfaceType interfaceSpecifier profileName

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Generates a GSMP port management message to the access node for the purpose of configuring a DSL profile string on the specified neighbor interface. There is no no version.

#### Options

- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- profileName—Name of profile to be used in the line configuration (port management) message

#### Mode

Global Configuration