# clear suspicious-control-flow-detection

#### Syntax

clear suspicious-control-flow-detection
[ interface interfaceSpecifier protocol protocolValue address ethernetAddress slot slotNumber ]

#### Release Information

Command introduced in JunosE Release 7.3.0.

#### Description

Clears one or more suspicious flows. If you do not specify a slot, interface, or IP address, clears all suspicious flows. If you specify a slot, clears all specified suspicious flows on that slot. If you specify an interface and protocol, clears flows that are identified down to the Ethernet mac address level. There is no no version.

#### Options

- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- protocolValue—Name of the protocol to be cleared
- ethernetAddress—Ethernet address to be cleared
- slotNumber—Number of the slot to be cleared

#### Mode

Privileged Exec, User Exec