# pppoe

#### Description

Point-to-Point over Ethernet layer

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

Error enabling control packet log

#### Warning Log

PPPoE interface or subInterface removed from NVS

#### Notice Log

PPPoE enabled; status change for subInterface

#### Info

Line module status change

#### Debug

Multiple PPPoE sessions with the same MAC address and containing the IWF-Session VSA in the PPPoE Active Discovery Request (PADR) packets are allowed; a PPPoE session with the IWF-Session VSA included in the PADR packets is established and terminated.

#### Filter

interface interfaceType interfaceSpecifier

- interface—Logs PPP events for a specific interface
- interfaceType—Type of interface for which you want to log PPP events
- interfaceSpecifier—Location of interface in the appropriate format

  | Note: For information about interface types and specifiers, see Interface Types and Specifiers in JunosE Command Reference Guide.