# aaa per-profile-attr-list (For Global Configuration)

#### Syntax

aaa per-profile-attr-list profileName action-type { enable | disable } attributes [ attributeName ]*

[ no ] aaa per-profile-attr-list profileName

#### Release Information

Command introduced in JunosE Release 12.1.0.

#### Description

Allows the user to configure an AAA per-profile list with attributes. The no version removes the configured AAA per-profile attribute list. By default, no attribute list is configured.

#### Options

- profileName—Name of the AAA per-profile; string of up to 32 characters
- enable—Includes the attribute in the request packets
- disable—Excludes the attribute in the request packets
- attributeName—The following AAA attributes can be specified:
  - tunnel-ignore-nasport
  - tunnel-ignore-nasport-type
  - *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

Global Configuration

#### Related Documentation

- Configuring an AAA Per-Profile Attribute List in the JunosE Broadband Access Configuration Guide