Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Example: QoS Parameter Configuration for QoS Downstream Rate
- For information about downstream rate and RADIUS, see JunosE Broadband Access Configuration Guide
- For more information about configuring ANCP (L2C) parameters, see JunosE IP Services Configuration Guide
- aaa qos downstream-rate
- controlled-interface-type
- encapsulation vlan
- instance-interface-type
- ip address
- node
- qos-parameter
- qos-adaptive-mode
- qos-parameter-define
- qos-profile
- queue
- shared-shaping-rate
- subscriber-interface-type
- traffic-class
- vlan id

# Configuring a Parameter Definition for QoS Downstream Rate

To associate a parameter instance with the QoS downstream rate application:

1. Configure traffic classes.
   host1(config)#traffic-class voice host1(config-traffic-class)#exit host1(config)#traffic-class best-effort host1(config-traffic-class)#exit
2. Create a parameter definition for the QoS downstream rate application.
   1. Configure the QoS parameter name and the application.
      host1(config)#qos-parameter-define downstreamVLAN application qos-downstream-rate
   2. Configure controlled-interface types.
      host1(config-qos-parameter-define)#controlled-interface-type vlan host1(config-qos-parameter-define)#controlled-interface-type ip
   3. Configure subscriber-interface types.
      host1(config-qos-parameter-define)#subscriber-interface-type vlan
3. Do one of the following:
   - For VLANs, configure the shaping mode by creating a parameter definition with the QoS cell mode application. Ensure that you specify a subscriber-interface type.

     See Configuring a Parameter Definition to Shape Ethernet Traffic Using Cell Mode.

   - For ATM VCs, configure the shaping mode by issuing the qos-shaping-mode command.

     See Configuring the QoS Shaping Mode for ATM Interfaces.

4. Enable QoS adaptive mode for the system by issuing the qos-adaptive-mode command in L2C Configuration mode.
   host1(config)#l2c host1(config-l2c)#qos-adaptive-mode
5. Enable the QoS downstream rate application to use downstream rates obtained from the Actual-Data-Rate-Downstream [26-130] DSL Forum VSA.
   host1(config)#aaa qos downstream-rate
6. Configure the scheduler profile for the shaping rate.
   host1(config)#scheduler-profile vlan1 host1(config-scheduler-profile)#shared-shaping-rate downstreamVLAN * 5 auto
7. Configure the QoS profile for the shaping rate.
   host1(config)#qos-profile vlan1 host1(config-qos-profile)#vlan node scheduler-profile vlan1
8. Attach the QoS profile to a logical Ethernet interface.

   ANCP or AAA dynamically creates the parameter instances for the QoS downstream rate application, and if applicable, the QoS cell mode application; therefore, you do not need to specify them.

   host1(config)#interface gigabitEthernet 6/0/2 host1(config-if)#encapsulation vlan host1(config-if)#interface gigabitEthernet 6/0/2.1 host1(config-if)#vlan id 1 host1(config-if)#qos-profile vlan1 host1(config-if)#ip address 6.10.10.10 255.255.255.255

## Related Documentation

- Example: QoS Parameter Configuration for QoS Downstream Rate
- For information about downstream rate and RADIUS, see JunosE Broadband Access Configuration Guide
- For more information about configuring ANCP (L2C) parameters, see JunosE IP Services Configuration Guide
- aaa qos downstream-rate
- controlled-interface-type
- encapsulation vlan
- instance-interface-type
- ip address
- node
- qos-parameter
- qos-adaptive-mode
- qos-parameter-define
- qos-profile
- queue
- shared-shaping-rate
- subscriber-interface-type
- traffic-class
- vlan id

#### Published: 2011-03-21

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out