Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# tx-connect-speed-method

#### Syntax

tx-connect-speed-method { static-layer2 | dynamic-layer2 | qos | actual }

no tx-connect-speed-method

#### Release Information

Command introduced in JunosE Release 8.0.0.

#### Description

Configures for an AAA domain map (when used from Domain Map Tunnel Configuration mode) or for an AAA tunnel group (when used from Tunnel Group Tunnel Configuration mode) the method used to calculate the transmit connect speed of the subscriber’s access interface for establishing a tunneled L2TP session. This speed is reported in L2TP Transmit (TX) Speed AVP 24. The no version removes configuration of the transmit connect speed calculation method from the AAA domain map or AAA tunnel group.

#### Options

- static-layer2—Calculates the transmit connect speed of the subscriber’s access interface based on statically configured settings for the underlying layer 2 interface
- dynamic-layer2—Calculates the transmit connect speed of the subscriber’s access interface based on dynamically configured settings for the underlying layer 2 interface
- qos—Calculates the transmit connect speed of the subscriber’s access interface based on settings determined by QoS
- actual—Calculates the transmit connect speed of the subscriber’s access interface as the lesser of the dynamic-layer2 value or the qos value

#### Mode

Domain Map Tunnel Configuration, Tunnel Group Tunnel Configuration

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out