# baseline frame-relay interface

#### Syntax

baseline frame-relay interface interfaceType interfaceSpecifier [ dlci ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets a statistics baseline for Frame Relay and MLFR interfaces, subinterfaces, and circuits. The router implements the baseline by reading and storing the statistics at the time the baseline is set and then subtracting this baseline whenever baseline-relative statistics are retrieved. There is no no version.

#### Options

- interfaceType—One of the following interface types listed in Interface Types and Specifiers
  - mlframe-relay
  - pos
  - serial
  - tunnel
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- dlci—DLCI number to be used on the specified subinterface to identify a virtual circuit in the range 16–1007

#### Mode

Privileged Exec