Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- show redundancy

# Monitoring the Redundancy Status

#### Purpose

Display the redundancy modes and other information about stateful SRP switchover.

#### Action

To display summary redundancy status information.

    host1#show redundancy

    SRP
    ---

    high-availability state:  disabled
    current redundancy mode:  high-availability
    last activation type:     cold-switch

    Criteria Preventing High Availability from being Active
    -------------------------------------------------------
                       criterion                      met
    -----------------------------------------------   ---
    Standby SRP is online and capable of mirroring?   No

    Line Card
    ---------

    automatic reverting is off

                                  backed
                                    up     sparing
           hardware    lockout      by       for     revert
    slot     role      config      slot     slot       at
    ----   --------   ---------   ------   -------   ------
     3       ---         ---       ---       ---      ---
     8      spare        ---       ---       ---      ---
     12    primary    protected    ---       ---      ---

             midplane   midplane
    slots      type       rev
    ------   --------   --------
    8 - 13      6          0

To display detailed redundancy status information:

    host1#show redundancy detail

    SRP
    ---

    high-availability state:  disabled
    current redundancy mode:  file-system-synchronization
    last activation type:     cold-start

       Criteria Required for High Availability to be Active
       ----------------------------------------------------
                         criterion                         met
    ----------------------------------------------------   ---
    Active SRP hardware supports High Availability?        Yes
    High Availability mode configured?                     No
    Mirroring Subsystem present?                           Yes
    Mirroring activity levels within limits?               Yes
    Network Core Dumps disabled?                           Yes
    Running configuration is safe for High Availability?   Yes
    Standby SRP hardware supports High Availability?       Yes
    Standby SRP is online and capable of mirroring?        Yes
    Standby SRP is running the same release?               Yes

    Line Card
    ---------

    automatic reverting is off

                                  backed
                                    up     sparing
           hardware    lockout      by       for     revert
    slot     role      config      slot     slot       at
    ----   --------   ---------   ------   -------   ------
     3       ---         ---       ---       ---      ---
     8      spare        ---       ---       ---      ---
     12    primary    protected    ---       ---      ---

             midplane   midplane
    slots      type       rev
    ------   --------   --------
    8 - 13      6          0

#### Meaning

Table 1 lists the show redundancy command output fields.

Table 1: show redundancy Output Fields

Field Name | Field Description
--- | ---
SRP
high-availability state | State of high availability mode: disabled—Initial, default state for high-availability mode. The router continues to use file system synchronization. active—Data synchronized from the active SRP module to the standby SRP module during initialization remains synchronized through mirroring updates. pending—If an unsupported application is configured, the router transitions to this state. initializing—If SRP module is in initializing state, bulk synchronization of memory and NVS occurs.
current redundancy mode | Redundancy mode currently used by the router: high-availability—Ensures rapid SRP module recovery after a switchover by using initial bulk file transfer and subsequent, transaction-based mirroring. file-system-synchronization—Default redundancy mode of the router. SRP modules reload all line modules and restart form saved configuration files.
last activation type | Last type of activation that occurred on the router. The method using which the SRP last booted: cold-switch—When the router is in pending state and switchover occurs, the router undergoes a cold-switch or cold re-start. warm-switch—When the router is in active state and switchover occurs, the router undergoes a warm-switch or warm re-start.
Criteria Preventing High Availability from being Active | Criteria preventing the router from being in the active state of high availability mode. Note: For the router to be in the Active state, all criteria for this option must be “yes”.
Criteria Required for High Availability to be Active | Criteria required for the router to be in the active state of high availability mode. Note: For the router to be in the Active state, all criteria for this option must be “yes”.
Line Card
automatic reverting | State of automatic reverting. Possible states: on or off.
slots | Slots in which the line modules reside.
hardware role | Function of the line module. Possible values: primary or spare.
lockout config | Status of redundancy on the line module: protected—Line module redundancy is enabled locked out—Line module redundancy is disabled
backed up by slot | Slot that contains the line module that is a spare for this primary line module.
sparing for slot | Slot that contains the primary line module for which this module is a spare.
revert at | Time at which you want the line module to revert.
midplane type | Identifier for the type of midplane.
midplane rev | Hardware revision number of the redundancy midplane.
fabric slice redundancy | Status of the fabric slice on the SRP modules or SFMs on the E120 and E320 routers.
slot | Slot in which the fabric slice resides.
slice state | State of the fabric slice. Possible values: online or not present.
type | Identifier for the type of hardware. Possible values: SRP modules or SFM modules.

## Related Documentation

- show redundancy

#### Published: 2011-03-24

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out