# clear ip interface

#### Syntax

clear ip interface [ vrf vrfName ] interfaceType interfaceSpecifier

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Clears the counters on the specified IP interface. The default is all interface types and all interfaces. There is no no version.

#### Options

- vrfName—Name of the VRF; string of 1–32 alphanumeric characters
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers

#### Mode

Privileged Exec