# bridge vpls site-range

#### Syntax

bridge vplsName vpls site-range siteRange

no bridge vplsName vpls site-range

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Configures the maximum number of customer sites that can participate in the specified VPLS domain that uses BGP as the signaling protocol. In a VPLS configuration, each customer site is represented by a customer edge (CE) device located at the edge of the customer's network. The router (VPLS edge device) communicates with the customer site by means of a bridge network interface connection to the CE device. The no version restores the default site range, 1.

The bridge vpls site-range command is not valid for a VPLS instance that uses LDP as the signaling protocol. To configure a VPLS instance with LDP signaling, use the mpls ldp vpls vpls-id command and the mpls ldp vpls neighbor command.

| Note: The bridge vpls site-range command is available for a VPLS instance only after you issue the bridge vpls transport-virtual-router command, which creates the VPLS instance and configures the transport virtual router.

#### Options

- vplsName—Name of a VPLS instance created with the bridge vpls transport-virtual-router command
- siteRange—Maximum number of sites that can participate in the VPLS domain, in the range 1–65534; default value is 1

#### Mode

Global Configuration

#### Related Documentation

- Configuring VPLS Instances with BGP Signaling in the JunosE BGP and MPLS Configuration Guide