# transmit-delay

#### Syntax

transmit-delay transmDelay

no transmit-delay

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets the estimated time it takes to transmit a link-state update packet on the OSPF remote-neighbor interface. The no version restores the default value.

#### Options

- transmDelay—Link-state transmit delay in seconds; a number in the range 0–3600; default value is 1

#### Mode

Remote Neighbor Configuration