# sscc update-policy-request enable

#### Syntax

[ no ] sscc update-policy-request enable

#### Release Information

Command introduced in JunosE Release 9.3.0.

#### Description

Configures the router to collect updated DSL line rate parameters from an access node using the ANCP topology discovery message and transmit the information to the COPS server with corresponding COPS messages. If you enable this feature, the access node sends line rate parameters not only during connection establishment, but also whenever any of the line rate values changes after the connection is built. The no version restores the default, which disables line rate parameters to be sent to the COPS server.

| Note: When you configure the sscc update-policy-request enable command, a warning message is displayed, prompting you to confirm whether you want to enable the router that functions as the SRC client to forcibly send updated line rate information parameters to the COPS server, which is running a release of SRC software earlier than Release 3.0.0 that is not compatible with the line rate message format.

#### Mode

Global Configuration

#### Related Documentation

- Configuring the SRC Client in the JunosE Broadband Access Configuration Guide
- Retrieval of DSL Line Rate Information from Access Nodes Overview