Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Clearing Dynamic MAC Addresses from the VPLS Forwarding Table in the JunosE BGP and MPLS Configuration Guide

# clear bridge interface

#### Syntax

clear bridge interface interfaceType interfaceSpecifier

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Removes from the forwarding table all dynamic (learned) MAC address entries for a specified network interface that belongs to a bridge group or to a VPLS instance . There is no no version.

| Note: Using the clear bridge interface command for a VPLS instance affects the specified network interface associated with the VPLS instance, but has no effect on the VPLS virtual core interface, which represents all of the MPLS tunnels from the router to the remote VPLS edge (VE) devices. To remove all MAC addresses from the forwarding table for the VPLS virtual core interface, use the clear bridge interface vpls command.

#### Options

- interfaceType—One of the following interface types listed in Interface Types and Specifiers
  - atm
  - fastEthernet
  - gigabitEthernet
  - tenGigabitEthernet
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers

#### Mode

Privileged Exec

## Related Documentation

- Clearing Dynamic MAC Addresses from the VPLS Forwarding Table in the JunosE BGP and MPLS Configuration Guide

#### Published: 2011-04-07

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out