# Unexpected AAA Authentication and Authorization Behavior During Unified ISSU

Authentication and command authorization are temporarily disabled on the serial console connection during the upgrade phase. You can connect to the serial console and issue the reload, show issu, and show version commands without the action of authentication and authorization servers, such as RADIUS or TACACS+.

#### Related Documentation

- Application Support for Unified ISSU