# Configuring WINS Primary and Secondary NMS

To configure the WINS primary and secondary name server addresses:

1. Specify the IP address of the WINS primary name server.
   host1(config)#aaa wins primary 192.168.10.05
2. Specify the IP address of the WINS secondary name server.
   host1(config)#aaa wins secondary 192.168.10.40

   | Note: The router uses name server addresses exclusively for PPP clients and not for domain name server resolution.