# show ethernet oam lfm status

#### Syntax

show ethernet oam lfm status interfaceType interfaceSpecifier

#### Release Information

Command introduced in JunosE Release 11.1.0.

#### Description

Displays the current Ethernet OAM link-fault management configuration for a particular interface. OAM must be operational on the interface when you run this command.

#### Options

- interfaceType—One of the following interface types listed in Interface Types and Specifiers:
  - fastEthernet
  - gigabitEthernet
  - tenGigabitEthernet
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers

#### Mode

Privileged Exec, User Exec

#### Related Documentation

- Monitoring OAM Link-Fault Management Configuration for an Interface