# mpls traffic-eng egress-label

#### Syntax

mpls { rsvp | traffic-eng } egress-label { non-null | explicit-null }

no mpls { rsvp | traffic-eng } egress-label

#### Release Information

Command introduced in JunosE Release 7.3.0.

#### Description

Specifies that the egress router advertises the explicit null label or a non-null label by means of RSVP-TE. See the mpls rsvp egress-label command for a complete description and syntax.

#### Mode

Global Configuration