# vlan auto-configure

#### Syntax

vlan auto-configure upperInterfaceType [ lockout-time { minTime maxTime |
none } ]

no vlan auto-configure upperInterfaceType [ lockout-time ]

#### Release Information

Command introduced in JunosE Release 7.1.0.
lockout-time keyword added in JunosE Release 7.3.0.

#### Description

Specifies the types of dynamic upper interface encapsulations that are accepted or detected by a dynamic VLAN subinterface. You can issue this command repeatedly in Profile Configuration mode to include autodetection of multiple upper interface encapsulation types within the base profile for a dynamic VLAN subinterface. The no version terminates detection of the specified encapsulation type.

#### Options

- upperInterfaceType—One of the following dynamic encapsulation types:
  - ip
  - pppoe
- minTime—Minimum lockout time in the range 1–86400 seconds (24 hours); default value is 1 second
- maxTime—Maximum lockout time in the range 1–86400 seconds (24 hours); default value is 1 second
- none—Disables lockout time for the specified dynamic encapsulation type

#### Mode

Profile Configuration