# mpls traffic-eng area

#### Syntax

[ no ] mpls traffic-eng area { areaId | areaIdInt }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables flooding of MPLS traffic-engineering link information into the specified OSPF area. Flooding is disabled by default. The no version disables flooding.

#### Options

- areaId—OSPF area ID in IP address format
- areaIdInt—OSPF area ID as a decimal value in the range 0–4294967295

#### Mode

Router Configuration