# SRP-10G Module Combination (2-GB Memory)

> Line module label | SRP-10G
> I/O module label | SRP I/O
> Number of I/O ports | 7
> Software release | First supported: 4.1.3 or later 4.1.x release, 5.0.4 or later 5.0.x release, 5.1.2 or higher-numbered release, 5.2.0 Final supported: Not applicable
> Description | 125 W Switch route processor (10 Gbps) Has a minimum of 2 GB of error checking and correction (ECC) memory with a 1-GB nonvolatile storage (NVS) card. The 512–MB version has reached end-of-life.
> Type | Not applicable
> Capability | Ethernet (IEEE 802.3) 10/100Base-T RS-232
> Software features | Not applicable
> Model compatibility | ERX710 Router ERX1410 Router
> SRP module compatibility | SRP-10G
> Module redundancy support | 1:1 redundancy
> Cables and connectors | Terminal blocks BNC, 75–ohm Wire wrap posts RJ-45 RS-232 (DB-9) See ERX Hardware Guide, Chapter 5, Cabling ERX Routers for more information.
> LEDs | See Module LEDs.
> Alarms, errors, and events | See Monitoring Modules in JunosE System Basics Configuration Guide, Chapter 6, Managing Modules.