# oam3ahEvents

#### Description

802.3 OAM link-fault management event details about problems detected on the link

#### Emergency

None

#### Alert

Link is disabled because the high threshold for an error is exceeded on the Ethernet OAM interface or because of the error-disable action specified to be performed in response to an OAM PDU received from a remote peer for a fault in the receive path of the link

#### Critical

None

#### Error

Link is disabled because the high threshold for an error is exceeded on the Ethernet OAM interface or because of the error-disable action specified to be performed in response to an OAM PDU received from a remote peer for a fault in the receive path of the link

#### Warning Log

None

#### Notice Log

None

#### Info

None

#### Debug

None

#### Filter

None