# frame-relay lmi-t392dce

#### Syntax

frame-relay lmi-t392dce seconds

no frame-relay lmi-t392dce

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets the polling verification timer (T392) on a DCE interface. The no version removes current setting and sets the default.

#### Options

- seconds—Number in the range 5–30 seconds; specifies the expected interval in seconds between status inquiries issued by the DTE equipment; default value is 15 seconds

#### Mode

Interface Configuration