# redundancy lockout

#### Syntax

[ no ] redundancy lockout slotNumber

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Prevents the router from switching automatically to a spare line module if the primary module fails on a slot. The no version reverts to the default situation, in which the router switches automatically to a spare line module if the primary module fails on a slot. The redundancy force-switchover command overrides this command.

#### Options

- slotNumber—Number of the slot in which the primary line module resides

#### Mode

Global Configuration