# send version

#### Syntax

[ no ] send version [ 1 | 2 | off ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Restricts the RIP version that the router can send on a remote-neighbor interface. The no version sets the remote-neighbor interface back to the default value, sending only RIP version 1.

#### Options

- 1—Specifies RIP version 1 only
- 2—Specifies RIP version 2 only
- off —Turns reception off

#### Mode

Remote Neighbor Configuration