# Monitoring Redundancy Status on E320 Router

#### Purpose

Display the configuration for line module redundancy and SRP module redundancy on an E320 router.

#### Action

    host1#show redundancy

    SRP
    ---

    high-availability state:  active
    current redundancy mode:  high-availability
    last activation type:     cold-start

    Criteria Preventing High Availability from being Active
    -------------------------------------------------------
                       criterion                      met
    -----------------------------------------------   ---
    Standby SRP is online and capable of mirroring?   No

    Line Card
    ---------

    automatic reverting is off

                                  backed
                                    up     sparing
           hardware    lockout      by       for     revert
    slot     role      config      slot     slot       at
    ----   --------   ---------   ------   -------   ------
     0       spare       ---       ---       ---      ---
     2     primary   protected     ---       ---      ---
     4     primary    protected    ---       ---      ---

    fabric slice redundancy : none

    slot      state        type
    ------   --------   --------
    6		    online      SFM-100
    7     	 online      SFM-100
    8       		---       ---
    9       		---       ---
    10       	---       ---

#### Meaning

Table 7 lists the show redundancy command output fields.

Table 7: show redundancy Output Fields

Field Name | Field Description
--- | ---
SRP
high-availability state | State of high availability mode: disabled—Initial, default state for high-availability mode. The router continues to use file system synchronization. active—Data synchronized from the active SRP module to the standby SRP module during initialization remains synchronized through mirroring updates. pending—If an unsupported application is configured, the router transitions to this state. initializing—If SRP module is in initializing state, bulk synchronization of memory and NVS occurs.
current redundancy mode | Redundancy mode currently used by the router: high-availability—Ensures rapid SRP module recovery after a switchover by using initial bulk file transfer and subsequent, transaction-based mirroring. file-system-synchronization—Default redundancy mode of the router. SRP modules reload all line modules and restart form saved configuration files.
last activation type | Last type of activation that occurred on the router. The method using which the SRP last booted: cold-start—When the router is in pending state and switchover occurs, the router undergoes a cold-start or cold switch. warm-start—When the router is in active state and switchover occurs, the router undergoes a warm switch or warm-start.
Criteria Preventing High Availability from being Active | Criteria preventing the router from being in the active state of high availability mode. Note: For the router to be in the Active state, all criteria for this option must be “yes”.
Criteria Required for High Availability to be Active | Criteria required for the router to be in the active state of high availability mode. Note: For the router to be in the Active state, all criteria for this option must be “yes”.
Line Card
automatic reverting | State of automatic reverting. Possible states: on or off.
slots | Slots in which the line modules reside.
hardware role | Function of the line module. Possible values: primary or spare.
lockout config | Status of redundancy on the line module: protected—Line module redundancy is enabled locked out—Line module redundancy is disabled
backed up by slot | Slot that contains the line module that is a spare for this primary line module.
sparing for slot | Slot that contains the primary line module for which this module is a spare.
revert at | Time at which you want the line module to revert.
midplane type | Identifier for the type of midplane.
midplane rev | Hardware revision number of the redundancy midplane.
fabric slice redundancy | Status of the fabric slice on the SRP modules or SFMs on the E120 and E320 routers.
slot | Slot in which the fabric slice resides.
slice state | State of the fabric slice. Possible values: online or not present.
type | Identifier for the type of hardware. Possible values: SRP modules or SFM modules.

#### Related Documentation

- show redundancy
- show redundancy line-card
- show redundancy srp