# redundancy revertive

#### Syntax

[ no ] redundancy revertive [ timeOfDay ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables the router to revert from spare line modules to available primary line modules automatically. The no version reverts to the default situation, in which there is no automatic reversion from spare to primary line modules.

#### Options

- timeOfDay—Time, in 24-hour format (00:00:00), at which the router reverts to the available primary line modules every day

#### Mode

Global Configuration