# snmp trap frame-relay link-status

#### Syntax

[ no ] snmp trap frame-relay link-status

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables processing of SNMP link status information about a Frame Relay major interface (if issued from Interface Configuration mode) or subinterface (if issued from Subinterface Configuration mode). The no version disables the processing of SNMP link status information.

#### Mode

Interface Configuration, Subinterface Configuration