# Monitoring the VRF Routing Table

#### Purpose

Display the routing table of the specified VRF

#### Action

To display the routing table of the VRF

    host1#show ip route vrf vpn2
    Protocol/Route type codes:
    I1- ISIS level 1, I2- ISIS level2,
    I- route type intra, IA- route type inter, E- route type external,
    i- metric type internal, e- metric type external,
    O- OSPF, E1- external type 1, E2- external type2,
    N1- NSSA external type1, N2- NSSA external type2

    Prefix/Length   Type     Next Hop    Dist/Met     Intf
    --------------- -------  ----------  --------      ------------
    45.5.5.5/32     Connect  45.5.5.5    0/1           fastEthernet3/0
    56.5.5.0/24     Connect  56.5.5.5    0/1           atm4/0.21

#### Meaning

Table 97 lists the show ip route command output fields.

Table 97: show ip route Output Fields

Field Name | Field Description
--- | ---
Protocol/Route type codes | Type of route
Prefix/Length | Network prefix for route in VRF routing table
Type | Protocol of route
Next Hop | IP address of the next hop to reach route
Dist/Met | Administrative distance and metric applied to route
Intf | Outgoing interface to reach route

#### Related Documentation

- show ip route