Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Configuring Interface Sets for QoS
- Configuring Interface Supersets for QoS

# qos-interface-parent

#### Syntax

In QoS Interface Set Configuration mode:

[ no ] qos-interface-parent interfaceSupersetName

In QoS Interface Superset Configuration mode:

[ no ] qos-interface-parent interface supersetInterfaceType interfaceSpecifier

In Interface Configuration mode:

[ no ] qos-interface-parent interfaceSetName

#### Release Information

Command introduced in JunosE Release 9.2.0.

#### Description

In QoS Interface Superset Configuration mode, assigns a parent interface for the interface superset. The parent interface can be an Ethernet major interface, an ATM major interface, or a LAG. The no version deletes the parent from the superset.

In QoS Interface Set Configuration mode, assigns a QoS interface superset as the parent for the interface set. The no version deletes the parent from the set.

In Interface Configuration mode, assigns a QoS interface set as the parent for the member interface. The no version deletes the parent from the interface.

#### Options

- interfaceSupersetName—Name of the QoS interface superset that is the parent of this interface set
- supersetInterfaceType—One of the following superset interface types: fastEthernet, gigabitEthernet, tenGigabitEthernet, atm, or lag
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- interfaceSetName—Name of the QoS interface set that is the parent of the interface

#### Mode

Interface Configuration, QoS Interface Set Configuration; QoS Interface Superset Configuration

## Related Documentation

- Configuring Interface Sets for QoS
- Configuring Interface Supersets for QoS

#### Published: 2011-04-01

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out