# radius per-profile-attr-list (For Global Configuration)

#### Syntax

radius per-profile-attr-list profileName request-type { access-request | acct-start | acct-stop } { enable | disable } attributes [ attributeName ]*

[ no ] radius per-profile-attr-list profileName

#### Release Information

Command introduced in JunosE Release 12.1.0.

#### Description

Allows the user to configure a RADIUS per-profile list with attributes. The no version removes the configured RADIUS per-profile attribute list. By default, no attribute list is configured.

#### Options

- profileName—Name of the RADIUS per-profile; string of up to 32 characters
- access-request—Configures RADIUS to include the attribute in Access-Request packets
- acct-start—Configures RADIUS to include the attribute in Acct-Start packets
- acct-stop—Configures RADIUS to include the attribute in Acct-Stop packets and Acct-Update message
- enable—Includes the attribute in the request packets
- disable—Excludes the attribute in the request packets
- attributeName—The following RADIUS attributes can be specified:
  - calling-station-id
  - override-nas-ip-addr
  - *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

Global Configuration

#### Related Documentation

- Configuring a RADIUS Per-Profile Attribute List in the JunosE Broadband Access Configuration Guide
- radius include
- radius override nas-ip-addr tunnel-client-endpoint