Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# ip vrf

#### Syntax

ip vrf vrfName

no ip vrf vrfName [ wait-for-completion [ waitSeconds ] ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Creates a VRF or accesses VRF Configuration mode to configure a VRF. The no version deletes the VRF.

| Note: After creating the VRF, you must configure a route distinguisher for it through the rd command. If the route distinguisher is not configured, the VRF cannot operate.

#### Options

- vrfName—Name of the VRF; a string of 1–32 alphanumeric characters
- wait-for-completion—Specifies (in the absence of waitSeconds) that the CLI waits for completion of the no version operation before it returns a prompt, regardless of how long that takes. Use the wait-for-completion keyword with the no version if you require a synchronous, deterministic deletion of a VRF, such as when executing Telnet or console commands by means of an external script. If you do not issue the wait-for-completion keyword in these circumstances, an ip vrf command issued as soon as the prompt appears might fail because the router is still deleting the VRF.
- waitSeconds—Number of seconds in the range 1–64000 that the CLI waits before it returns a prompt, regardless of whether the no version operation has completed

#### Mode

Global Configuration

#### Published: 2011-04-07

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out